Interface Fa0/1 of Switch 1 is configured as an access port.

Change it to trunk port so that traffic can be passed successfully between two switches.