When we are pinging one pc from another, Fa 0/2 on switch is shutting down.

Troubleshoot the issue.