Subinterface FA0/0.10 on router is configured to respond to Vlan 50 traffic but Vlan 50 does not exist in this lab.

Correct the configuration so that interface should respond to Vlan 10 traffic to solve the issue.