CDP is disabled on the interface serial 0/0/0 on Router2, enable the CDP on the mentioned interface to solve the issue.

Go to the interface configuration mode and type CDP enable.