VTP is configured as client mode on the switch, VTP client does not have ability to create Vlans.

To configure vlan on the switch, change the VTP mode on the switch to VTP server or transparent.

Use command from global configuration mode (VTP mode server) or (VTP mode transparent)