Add command [permit any] rule in the access list 1 because there is always a hidden deny all at the end of the access list so we have to permit the other traffic.

By default, if we do not permit allowed traffic then access list will block all traffic.